# TURN Server Configuration (coturn)
# Copy to /etc/turnserver.conf

# Ports
listening-port=3479
tls-listening-port=5350
listening-ip=0.0.0.0

# External IP for NAT traversal
# Format: external-ip=<public-ip>/<internal-ip>
external-ip=YOUR_WAN_IP/192.168.0.154

# Authentication
fingerprint
use-auth-secret
static-auth-secret=<TURN_SHARED_SECRET>
realm=matrix.thevish.io

# Quotas
total-quota=100
bps-capacity=0
stale-nonce=600

# Security
no-multicast-peers

# Media relay ports (must be forwarded through firewall)
min-port=49201
max-port=49250

# Logging
log-file=/var/log/turnserver.log
verbose
